# Excelitas PCO GmbH   -     TECHNICAL  INFORMATION  DOCUMENT


# VERSION HISTORY

Version 1.9.0.0:
------------------------------
- Ensure automatic fan target temperature setting
- Bugfixes

Version 1.8.0.1:
------------------------------
- support Get/SetCameraSetup to configure Pixelformat

Version 1.7.0.12:
------------------------------
- bugfix sizes in GetCameraDescription
- delayload genicam dll's
- correct values in default descriptor

Version 1.6.1.4:
------------------------------
- bugfix: ROI setting with offset change descriptor

Version 1.6.0.0:
------------------------------
- correct GenICam masks for error codes

Version 1.5.1.0:
------------------------------
- bugfix: revoke busy state buffers on acquisition stop
- update PCO.cti producer (1.1.27)
- right polarity for Acq. enable signal
- display name: pco.pixelfly 1.3 SWIR
- link correction data download tool in message box
- add values for firmware versions

Version 1.5.0.0:
------------------------------
- fix multi process access for multiple cameras
- optionally suppress message box for missing correction data

Version 1.4.0.89:
------------------------------
- First release
- Interface to access GenICam GenTL Producer PCO.cti (1.1.23) from ABS. 
- Wrapping GenICam features and routines to sc2 telegrams (pco.sdk 1.28.*)

```
 Excelitas PCO GmbH
 DONAUPARK 11
 93309 KELHEIM / GERMANY
 PHONE +49 (9441) 20050
 FAX   +49 (9441) 200520
 info@pco.de, support@pco.de
 http://www.pco.de
``` 
```
 DISCLAIMER
 THE ORIGIN OF THIS INFORMATION MAY BE INTERNAL OR EXTERNAL TO PCO.
 PCO MAKES EVERY EFFORT WITHIN ITS MEANS TO VERIFY THIS INFORMATION.
 HOWEVER, THE INFORMATION PROVIDED IN THIS DOCUMENT IS FOR YOUR
 INFORMATION ONLY. PCO MAKES NO EXPLICIT OR IMPLIED CLAIMS TO THE
 VALIDITY OF THIS INFORMATION.
-------------------------------------------------------------------
 Any trademarks referenced in this document are the property of
 their respective owners.
```
